|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
|  |
| OnetheTwo punch leak detection testGaussan HV AND LV Vector MappingThe Gaussan™ electronic leak detection method pinpoints all penetrations in the waterproofing envelope. Using the High Voltage sweep before the Low Voltage Vector Mapping is by far the most complete way to test and it ensures that you can walk away from your job with total confidence without paying any extra. Our quotes always include the use of both methods where applicable. Call us to bid your next project |
|  |

 |  |

|  |
| --- |
| The Complete Way to Test Over 30 years of Membrane Testing ExperienceTimely Detailed Field ReportsLV Vector Mapping Testing System Always Permanently InstalledReal-Time Leak Detection Systems |
|  |
| 603-286-1942931-446-3012 |

 |